FederalRegister
Technology, Trade, Legal, Regulatory Policy and Standards Related Notices   -  August 11  - August 25 ,  2005
Compiled under ANSI contract from on line  database  by GTWAssociates 
	Topic	Special Conditions: Boeing Model 747-400 Airplane; Large Non-
	Structural Glass in the Passenger Compartment
	Date-Document-Sources 	8/11/2005	05–15856	DOT	TEXT	PDF
	 Standard  Ref	ANSI/SAE Z26.1 section 5.7, Test 7
	 Discussion 	This action proposes special conditions for a Boeing Model 
	747-400 airplane modified by Lufthansa Technik AG. This airplane will 
	have a novel or unusual design feature associated with the installation 
	of large non-structural glass items in the cabin area of an executive 
	 Note 	 For large glass components mounted in a cabin occupied by 
	passengers or crew that are not otherwise protected from the injurious 
	effects of failure of the glass component, the following apply:
	    Material. The glass used must be tempered or otherwise treated to 
	Topic	Codex Alimentarius Commission: Meeting of the Codex Committee on 
	Nutrition and Foods for Special Dietary Uses
	Date-Document-Sources 	8/11/2005	05–15913	FDA	TEXT	PDF
	 Standard  Ref	Recommendations on the Scientific Basis of Health Claims.
	 Discussion 	The Office of the Under Secretary for Food Safety, United 
	States Department of Agriculture (USDA), and the Food and Drug 
	Administration (FDA), U.S. Department of Health and Human Services 
	(HHS), are sponsoring a public meeting on October 18, 2005. The 
	 Note 	 Codex was established in 1962 by two United Nations organizations, 
	the Food and Agriculture Organization (FAO) and the World Health 
	Organization (WHO). Codex is the major international organization for 
	encouraging fair international trade in food and protecting the health 
	Topic	Federal Motor Vehicle Safety Standards; Bus Emergency Exits and 
	Window Retention and Release
	Date-Document-Sources 	8/12/2005	05–16016	SAE	TEXT	PDF
	 Standard  Ref	voluntary consensus standards bodies, such as the Society of Automotive 
	Engineers (SAE).
	 Discussion 	SUMMARY: This document responds to petitions for reconsideration of an 
	April 19, 2002 final rule amending Federal Motor Vehicle Safety 
	Standard No. 217, ``Bus emergency exits and window retention and 
	release.'' That final rule amended the standard to reduce the 
	 Note 	Section 12(d) of the National Technology Transfer and Advancement 
	Act of 1995 (NTTAA), Public Law 104-113, section 12(d) (15 U.S.C. 272) 
	directs us to use voluntary consensus standards in our regulatory 
	activities unless doing so would be inconsistent with applicable law or 
	Topic	Advisory bulletins— 
	 Manufacture, marking, and sale of substandard compressed gas cylinders
	Date-Document-Sources 	8/12/2005	05–16022	DOT	TEXT	PDF
	 Standard  Ref	DOT-E 12695 has been suspended
	 Discussion 	This is to notify the public that PHMSA and the Office of the 
	Inspector General (OIG) are investigating the manufacture, marking, and 
	sale of high pressure DOT exemption cylinders made and/or distributed 
	by Global Composites International, Inc. (GCI), Ontario, CA. PHMSA and 
	 Note 	Through its investigation, PHMSA and the OIG 
	believe that GCI manufactured, marked, certified and sold an 
	undetermined number of high-pressure carbon fiber wrapped cylinders 
	owned by commercial entities and the private consumer. Among others, we 

	Topic	Certain Corrosion-Resistant Carbon Steel Flat Products From 
	Japan:
	Date-Document-Sources 	8/15/2005	E5–4408	DOC	TEXT	PDF
	 Standard  Ref	SAE standard 792 for Bearing and Bushing Alloys; carbon steel coil (SAE 1008)
	 Discussion 	Department'') published a notice of initiation of a changed 
	circumstances review regarding certain corrosion-resistant carbon steel 
	flat products from Japan in response to a request for partial 
	revocation received from Metal One Corporation (``Metal One''), and 
	 Note 	lso excluded from the scope of this order are: (1) Carbon steel 
	flat products measuring 1.84 mm in thickness and 43.6 mm or 16.1 mm in 
	width consisting of carbon steel coil (SAE 1008) clad with an aluminum 
	alloy that is balance aluminum, 20% tin, 1% copper, 0.3% silicon, 0.15% 
	Topic	International Telecommunication Advisory Committee,
	Date-Document-Sources 	8/15/2005	05–16127	DOS	TEXT	PDF
	 Standard  Ref	World Summit on the Information Society
	 Discussion 	United States International Telecommunication Advisory Committee 
	Information Meeting on the World Summit on the Information Society; 
	Notice of Meeting
	
	 Note 	The ITAC will meet to discuss the matters related to the second 
	phase of the World Summit on the Information Society (WSIS), in 
	preparation for the third WSIS Preparatory Committee Meeting. The 
	meeting will take place on Thursday, September 8, 2005, from 10:30 a.m. 
	Topic	Parts and Accessories Necessary for Safe Operation; General 
	Amendments
	Date-Document-Sources 	8/15/2005	05–14259	Federal Motor Carrier Safety	TEXT	PDF
	 Administration
	 Standard  Ref	removal of references to the Society of Automotive Engineers' (SAE) standards would have an 
	adverse impact on safety
	 Discussion 	FMCSA amends part 393 of the Federal Motor Carrier Safety 
	Regulations (FMCSRs), Parts and Accessories Necessary for Safe 
	Operation. The amendments are intended to remove obsolete and redundant 
	regulations; respond to several petitions for rulemaking; provide 
	 Note 	On March 24, 1998, FHWA held a public meeting to discuss 
	requirements for brake hoses used on commercial motor vehicles. An 
	announcement of the meeting was published in the Federal Register on 
	February 20, 1998 (63 FR 8606). Several brake hose manufacturers 
	Topic	New Standards for Periodicals Mail Prepared in Sacks
	Date-Document-Sources 	8/15/2005	05–16200	POSTAL SERVICE	TEXT	PDF
	 Standard  Ref	mailing industry are working together to control costs. We can reduce 
	the costs of transporting and processing mail in sacks by requiring 
	 Discussion 	We are proposing new standards to reduce handling costs for 
	Periodicals mail prepared in sacks. Our proposal includes the following 
	changes: two new types of sacks: a 3-digit carrier routes sack and a 
	merged 3-digit sack; and a new minimum of 24 pieces for most other 
	 Note 	  [Revise 9.2.4 by adding a reference to 24 pieces to read as 
	follows:]
	    5-digit and 3-digit bundles prepared under 707.22.0 and 707.25.0 or 
	under 9.2.3 may contain fewer than six pieces when the publisher 

	Topic	Office of State and Local Government Coordination and 
	Preparedness
	Date-Document-Sources 	8/16/2005	05–16309	DHS	TEXT	PDF
	 Standard  Ref	2004 survey by the National Fire Protection Association (NFPA),
	 Discussion 	The Department of Homeland Security is publishing this Notice 
	to provide details and guidance regarding the 2005 program year 
	Assistance to Firefighters Grant Program. The program makes grants 
	directly to fire departments and nonaffiliated emergency medical 
	 Note 	Under the provisions of 15 U.S.C. 2229a, DHS must ensure that fire 
	departments that have either all-volunteer forces of firefighting 
	personnel or combined forces of volunteer and career firefighting 
	personnel receive a portion of the total grant funding that is not less 
	Topic	Irradiation in the Production, Processing, and Handling of Food
	Date-Document-Sources 	8/16/2005	05–16279	FDA	TEXT	PDF
	 Standard  Ref	Codex 2003, ``Codex General Standard for Irradiated Foods 
	(CODEX STAN 106-1983, Rev.-2003)
	 Discussion 	The Food and Drug Administration (FDA) is amending the food 
	additive regulations to provide for the safe use of ionizing radiation 
	for control of Vibrio species and other foodborne pathogens in fresh or 
	frozen molluscan shellfish (e.g., oysters, mussels, clams, etc.). This 
	 Note 	    The comment states that the petition should be denied because ``[a] 
	majority of Parliamentary Members voted for a provision that the EU's 
	list of foods authorised (sic) for irradiation should not be 
	expanded,'' and ``[a] working group of the Codex Alimentarius 
	Topic	Biweekly Notice Applications and Amendments to Facility Operating 
	Licenses Involving No Significant Hazards Considerations
	Date-Document-Sources 	8/16/2005	E5–4403	NRC	TEXT	PDF
	 Standard  Ref	American Society of Mechanical Engineers (ASME) Code 
	frequency for testing these valves
	 Discussion 	Pursuant to section 189a. (2) of the Atomic Energy Act of 1954, as 
	amended (the Act), the U.S. Nuclear Regulatory Commission (the 
	Commission or NRC staff) is publishing this regular biweekly notice. 
	The Act requires the Commission publish notice of any amendments 
	 Note 	Basis for proposed no significant hazards consideration 
	determination: As required by 10 CFR 50.91(a), the licensee has 
	provided its analysis of the issue of no significant hazards 
	consideration, which is presented below:
	Topic	High Island Offshore System, L.L.C.; Notice of Compliance Filing
	Date-Document-Sources 	8/16/2005	E5–4443	FERC	TEXT	PDF
	 Standard  Ref	Wholesale Gas Quadrant (WGQ) of the North American Energy Standards 
	Board (NAESB).
	 Discussion 	Take notice that on July 29, 2005, High Island Offshore System, 
	L.L.C. (HIOS) tendered for filing as part of its FERC Gas Tariff, Third 
	Revised Volume No. 1, Substitute Eighth Revised Sheet No. 170, to be 
	made effective September 1, 2005.
	 Note 	 Take notice that on July 29, 2005, High Island Offshore System, 
	L.L.C. (HIOS) tendered for filing as part of its FERC Gas Tariff, Third 
	Revised Volume No. 1, Substitute Eighth Revised Sheet No. 170, to be 
	made effective September 1, 2005.

	Topic	Guidelines Establishing Test Procedures for the Analysis of 
	Pollutants; Analytical Methods for Biological Pollutants in Wastewater 
	Date-Document-Sources 	8/16/2005	05–16195	EPA	TEXT	PDF
	 Standard  Ref	 ASTM   D6503-99  AOAC. 1995. Official Methods of Analysis of AOAC I
	 Discussion 	This proposed regulation would amend the ``Guidelines 
	Establishing Test Procedures for the Analysis of Pollutants'' under 
	section 304(h) of the Clean Water Act (CWA), by adding analytical test 
	procedures for enumerating the bacteria, Escherichia coli (E. coli) and 
	 Note 	Membrane Filter (MF) Test for Enterococci: mEI Agar (EPA Method 
	1600). The mE-EIA agar method is a two-step MF procedure that provides 
	a direct count of bacteria in water, based on the development of 
	colonies on the surface of a filter when placed on selective mE agar 
	Topic	Request for Information on New Commercial Vehicle Safety 
	Inspection Concepts
	Date-Document-Sources 	8/16/2005	05–16163	FMCSA	TEXT	PDF
	 Standard  Ref	concepts that will improve commercial vehicle safety
	 Discussion 	FMCSA invites comments, suggestions and creative ideas on new 
	operational concepts that will improve commercial vehicle safety 
	inspections through more thorough performance-based inspections. 
	Commercial vehicle roadside safety inspections represent one of the 
	 Note 	Statistics show there are 8 million trucks and buses that travel 
	208 billion miles on our nation's highways each year, and commercial 
	vehicle miles traveled are forecasted to grow approximately 2 percent 
	annually. In addition, truck traffic will increase approximately 25 
	Topic	Strategic Approach to International Chemicals Management; Third Preparatory Committee
	Date-Document-Sources 	8/17/2005	05–16299	EPA	TEXT	PDF
	 Standard  Ref	    Environmental protection, Chemicals, Hazardous materials 
	transportation, Hazardous substances, Public health, Safety.
	 Discussion 	This notice announces that EPA and the State Department are 
	hosting a meeting for stakeholders to inform the development of the 
	U.S. Government's viewpoints for the upcoming 3\rd\ Preparatory 
	Committee (PrepComm 3) meeting on the Strategic Approach to 
	 Note 	    This action is directed to the public in general, and may be of 
	particular interest to industry, trade associations, and non-
	governmental organizations that deal with and are interested in 
	international chemicals management. If you have any questions regarding 
	Topic	Federal Motor Vehicle Safety Standards; Low Speed Vehicles
	Date-Document-Sources 	8/17/2005	05–16323	NHTSA	TEXT	PDF
	 Standard  Ref	standards SAE J-2358, ISO 391-6:2003, and ASME 56.8)
	 Discussion 	This final rule amends the definition of ``low-speed vehicle'' 
	(LSV) in two ways. First, it eliminates the exclusion of trucks from 
	that class of vehicles. Second, it limits the class of LSVs to those 
	vehicles with a Gross Vehicle Weight Rating (GVWR) of less than 1,134 
	 Note 	 Two commenters, NGCMA and Advocates, opposed removing the truck 
	exclusion from the definition of LSV. NGCMA asserted that NHTSA failed 
	to consider numerous industry standards concerning LSV performance and 
	safety (specifically standards SAE J-2358, ISO 391-6:2003, and ASME 

	Topic	Motor vehicle safety standards: 
	  Controls, telltales, and indicators,
	Date-Document-Sources 	8/17/2005	05–16325	NHTSA	TEXT	PDF
	 Standard  Ref	Harmonizing With Canadian and International Standards United Nations/Economic 
	Commission for Europe World Forum for Harmonization of Vehicle 
	 Discussion 	In this document, we update our standard regulating motor 
	vehicle controls, telltales and indicators. The standard specifies 
	requirements for the location, identification, and illumination of 
	these items. This rule extends the standard's telltale and indicator 
	 Note 	Another topic of the NPRM was international harmonization of 
	controls and displays standards. NHTSA consulted with Transport Canada 
	(Canada's counterpart to the U.S. Department of Transportation) in the 
	late 1990s about Canada's controls and displays standard, i.e., 
	Topic	Environmental Technologies Trade Advisory Committee
	Date-Document-Sources 	8/17/2005	E5–4487	ITA	TEXT	PDF
	 Standard  Ref	Environmental 
	Technologies Verification (ETV) Program
	 Discussion 	The Environmental Technologies Trade Advisory Committee 
	(ETTAC) will hold a plenary meeting on September 16, 2005, at the U.S. 
	Department of Commerce, 14th Street and Constitution Avenue, NW., 
	Washington, DC 20230, in Room 4830. The ETTAC will discuss global 
	 Note 	The afternoon session will include a discussion of the 
	U.S. EPA's Resource Conservation Challenge, the Environmental 
	Technologies Verification (ETV) Program and an overview of the U.S. 
	International Trade Commission's environmental services sector market 
	Topic	Identification Requirements for Buses Manufactured in Two or More 
	Stages
	Date-Document-Sources 	8/18/2005	05–16324	NHTSA	TEXT	PDF
	 Standard  Ref	information to be included on a certification label American Society for Testing and Materials 
	(ASTM), 
	 Discussion 	This document proposes to amend Part 567 to require that, in 
	addition to the vehicle identification number, additional information 
	be recorded on the certification label of each bus manufactured in two 
	or more stages. The information would identify the bus body 
	 Note 	Section 12(d) of the National Technology Transfer and Advancement 
	Act (NTTAA) requires NHTSA to evaluate and use existing voluntary 
	consensus standards \3\ in its regulatory activities unless doing so 
	would be inconsistent with applicable law (e.g., the statutory 
	Topic	survey up to 3,700 consumers
	Date-Document-Sources 	8/19/2005	05–16464	FTC	TEXT	PDF
	 Standard  Ref	incidence of consumer fraud in the general 
	population
	 Discussion 	In 2003, OMB approved the FTC's request to 
	conduct a survey on consumer fraud and assigned OMB Control Number 
	3084-0125. The FTC completed the consumer research in June 2003 and 
	issued its report, Consumer Fraud in the United States: An FTC Survey, 
	 Note 	The FTC proposes to survey up to 3,700 consumers in order to gather 
	specific information on the incidence of consumer fraud in the general 
	population.\3\ All information will be collected on a voluntary basis, 
	and the identities of the consumers will remain confidential. Subject 

	Topic	Federal Motor Vehicle Safety Standards; Seat Belt Assemblies
	Date-Document-Sources 	8/22/2005	05–16524	NHTS	TEXT	PDF
	 Standard  Ref	Society of Automotive Engineers (SAE) Recommended Practice J211-1 rev. December 2003
	 Discussion 	This final rule amends the Federal motor vehicle safety 
	standard (FMVSS) for seat belt assemblies to redefine the requirements 
	and to establish a new test methodology for emergency-locking 
	retractors. Specifically, this final rule establishes a new 
	 Note 	 After careful consideration of all available information, including 
	public comments, the agency has decided to retain in this final rule 
	the approach set forth in the NPRM, with minor technical modifications. 
	All such modifications and the accompanying rationale are discussed 
	Topic	Participating Countries and Entities (Hereinafter Known as ``Participants'') Under the Clean Diamond 
	Trade 
	Date-Document-Sources 	8/22/2005	05–16602	DOS	TEXT	PDF
	 Standard  Ref	Kimberley Process Certification Scheme
	 Discussion 	Section 4 of the Clean Diamond Trade Act 
	(the ``Act'') requires the President to prohibit the importation into, 
	or the exportation from, the United States of any rough diamond, from 
	whatever source, that has not been controlled through the Kimberley 
	 Note 	Section 6(b) of the Act requires the President to publish in the 
	Federal Register a list of all Participants, and all Importing and 
	Exporting Authorities of Participants, and to update the list as 
	necessary. Section 2 of Executive Order 13312 of July 29, 2003 
	Topic	Southern Nuclear Operating Company, Inc.; Notice of Consideration 
	of Issuance of Amendment
	Date-Document-Sources 	8/22/2005	E5–4554	NRC	TEXT	PDF
	 Standard  Ref	consistent with the requirements of 
	Section III of the American Society of Mechanical Engineers (ASME
	 Discussion 	The U.S. Nuclear Regulatory Commission (the Commission) is 
	considering issuance of amendments to Facility Operating License Nos. 
	NPF-68 and NPF-81 issued Southern Nuclear Operating Company, Inc. 
	(SNC), for operation of the Vogtle Electric Generating Plant (VEGP), 
	 Note 	 Does the proposed amendment involve a significant reduction 
	in a margin of safety?
	    No. The proposed changes maintain the required structural 
	margins of the SG tubes for both normal and accident conditions. 
	Topic	Unregulated Contaminant Monitoring Regulation (UCMR) for Public Water 
	Systems Revisions; Proposed Rule
	Date-Document-Sources 	8/22/2005	05–16385	EPA	TEXT	PDF
	 Standard  Ref	Standard Methods, Association of Analytical Communities International, and American Society 
	for Testing 
	 Discussion 	The Safe Drinking Water Act (SDWA), as amended in 1996, 
	requires the United States Environmental Protection Agency (EPA) to 
	establish criteria for a program to monitor unregulated contaminants 
	and to publish a list of contaminants to be monitored every five years. 
	 Note 	National Technology Transfer and Advancement Act
	
	    Section 12(d) of the National Technology Transfer and Advancement 
	Act of 1995 (NTTAA), Public Law 104-113, Section 12(d) (15 U.S.C. 272 

	Topic	Federal Motor Vehicle Safety Standards; Roof Crush Resistance
	Date-Document-Sources 	8/23/2005	05–16661	NHTSA	TEXT	PDF
	 Standard  Ref	evaluated the Society of Automotive Engineers (SAE) inverted drop testing procedure,
	 Discussion 	As part of a comprehensive plan for reducing the serious risk 
	of rollover crashes and the risk of death and serious injury in those 
	crashes, this document proposes to upgrade the agency's safety standard 
	on roof crush resistance in several ways. First, we are proposing to 
	 Note 	Under the National Technology Transfer and Advancement Act of 1995 
	(NTTAA) (Pub. L. 104-113), ``all Federal agencies and departments shall 
	use technical standards that are developed or adopted by voluntary 
	consensus standards bodies, using such technical standards as a means 
	Topic	Southern Nuclear Operating Company, Joseph M. Farley Nuclear 
	Power Plant, Units 1 and 2; Exemption
	Date-Document-Sources 	8/23/2005	E5–4597	NRC	TEXT	PDF
	 Standard  Ref	NRC has adopted National Fire Protection Association Standard 805, 2001 Edition (NFPA 805),
	 Discussion 	The Southern Nuclear Operating Company (SNC, the licensee) is the 
	holder of Renewed Facility Operating License Nos. NPF-2 and NPF-8 which 
	authorizes operation of Joseph M. Farley Nuclear Power Plant (FNP), 
	Units 1 and 2. The license provides, among other things, that the 
	 Note 	For this specific fire protection application, SNC proposes plant 
	and fire protection program modifications under FNP's current license 
	conditions, and has performed deterministic re-analyses and a risk-
	informed, performance-based evaluation to revise existing Exemption 
	Topic	Federal Motor Vehicle Safety Standards; Occupant Crash 
	Protection; Anthropomorphic Test Devices
	Date-Document-Sources 	8/23/2005	05–16721	NHTSA	TEXT	PDF
	 Standard  Ref	SAE Paper 1999-01-007
	 Discussion 	On February 3, 2004, NHTSA published a notice in the Federal 
	Register requesting comments on whether to propose adding a high speed 
	frontal offset crash test to Federal Motor Vehicle Safety Standard 
	(FMVSS) No. 208, ``Occupant crash protection.'' The notice informed the 
	 Note 	Summers, Prasad, Hollowell, `` NHTSA's Vehicle 
	Compatibility Research Program,'' SAE Paper 1999-01-0071, SAE 
	International Congress and Exposition, Detroit, MI, 1999.Furthermore, our concerns were 
	reinforced by vehicle manufacturers' 
	Topic	Certification Requirements for Imported Natural Wine (2005R-002P)
	Date-Document-Sources 	8/24/2005	05–16771	DOTr	TEXT	PDF
	 Standard  Ref	certification requirements regarding production practices and procedures for imported natural 
	wine
	 Discussion 	 Elsewhere in this issue of the Federal Register, the Alcohol 
	and Tobacco Tax and Trade Bureau is issuing a temporary rule 
	implementing the new certification requirements regarding production 
	practices and procedures for imported natural wine contained in section 
	 Note 	We request comments from everyone interested. We are particularly 
	interested in comments on the effect these regulatory requirements 
	might have on U.S. importers who do not obtain their wine directly from 
	foreign producers, and we would welcome any suggestions for alternative 

	Topic	Certification Requirements for Imported Natural Wine (2005R-002P)
	Date-Document-Sources 	8/24/2005	05–16772	DOTr	TEXT	PDF
	 Standard  Ref	certification requirements regarding production practices and procedures for imported 
	natural wine
	 Discussion 	This temporary rule implements the new certification 
	requirements regarding production practices and procedures for imported 
	natural wine contained in section 2002 of the Miscellaneous Trade and 
	Technical Corrections Act of 2004, which amended section 5382 of the 
	 Note 	 In the case of an importer that owns or controls or that has an 
	affiliate that owns or controls a winery operating under a basic permit 
	issued by the Secretary, the importer certifies that the practices and 
	procedures used to produce the wine constitute proper cellar treatment 
	Topic	National Emissions Standards for Hazardous Air Pollutants: 
	Reinforced Plastic Composites Production
	Date-Document-Sources 	8/25/2005	05–16701	EPA	TEXT	PDF
	 Standard  Ref	High Performance gel coat means a gel coat used on products for 
	which National Sanitation Foundation, United States Department of 
	 Discussion 	The EPA is taking direct final action on amendments to the 
	national emissions standards for hazardous air pollutants (NESHAP) for 
	reinforced plastic composites production which were issued April 12, 
	2003, under section 112 of the Clean Air Act (CAA). The direct final 
	 Note 	High Performance gel coat means a gel coat used on products for 
	which National Sanitation Foundation, United States Department of 
	Agriculture, ASTM, durability, or other property testing is required.
	* * * * *
	Topic	Criteria for Accident Monitoring Instrumentation for Nuclear Power Plants
	Date-Document-Sources 	8/25/2005	E5–4647	NRC	TEXT	PDF
	 Standard  Ref	Institute of Electrical and Electronics Engineers (IEEE) promulgated as 
	IEEE Std. 497-2002
	 Discussion 	U.S. Nuclear Regulatory Commission (NRC) has issued for public 
	comment a draft revision to an existing guide in the agency's 
	Regulatory Guide Series. This series has been developed to describe and 
	make available to the public such information as methods that are 
	 Note 	This proposed revision of Regulatory Guide 1.97 represents an 
	ongoing evolution in the nuclear industry's thinking and approaches 
	with regard to accident monitoring systems for the Nation's nuclear 
	power plants. Specifically, this revision endorses (with certain 
	Topic	General Motors Corporation, Grant of Petition for Decision of 
	Inconsequential Noncompliance
	Date-Document-Sources 	8/25/2005	05–16862	NHTSA	TEXT	PDF
	 Standard  Ref	Section 7 of ANSI/SAE Z26.1-1996
	 Discussion 	General Motors Corporation (General Motors) has determined that 
	certain model year 2005 vehicles that it produced do not comply with S6 
	of 49 CFR 571.205, Federal Motor Vehicle Safety Standard (FMVSS) No. 
	205, ``Glazing materials.'' Pursuant to 49 U.S.C. 30118(d) and 
	 Note 	Affected are a total of approximately 7,326 model year 2005 
	Chevrolet Corvette coupes equipped with removable transparent Targa 
	roofs. S6, certification and marking, of FMVSS No. 205 and the 
	referenced Section 7 of ANSI/SAE Z26.1-1996 specify that the required 

	Topic	Water quality standards; designated uses and use attainability analyses; public meeting
	Date-Document-Sources 	8/25/2005	05–16928	EPA	TEXT	PDF
	 Standard  Ref	Water quality standards
	 Discussion 	The Environmental Protection Agency (EPA) is holding a public 
	meeting to discuss designated uses and use attainability analyses. The 
	meeting is co-sponsored with the Water Environment Federation (WEF). 
	The primary goals of the meeting are to help educate the public on 
	 Note 	The purpose of this public meeting is to 
	help educate the public on current water quality standards regulations, 
	guidance and practices related to designated uses and use attainability 
	analyses, and to provide a forum for the public to join in discussions,